**Software Installation Prerequisite**

1. Download and install the latest Python release: <https://www.python.org/downloads/>
2. During installation setup, confirm the following boxes are checked:
3. “Add Python x.x to Path”
4. “pip (download and install other Python packages)”
5. Confirm that the Windows Path environment variable contains a pointer to the Python installation directory. For example, if Python was installed into C:\Python, the Path variable should include it

Graphical user interface, text, application, email

Description automatically generated

1. Open a command line window (e.g. Command Prompt or PowerShell)
2. Navigate to the main “sam-iot-provision” folder

> cd [path]\sam-iot-provision

1. Install the required Python modules needed by the tool’s scripts:

> python -m pip install --upgrade pip

> pip install -r py\_modules.txt

(if this step fails, you may need to install Microsoft Visual Studio from <https://visualstudio.microsoft.com/downloads/#build-tools-for-visual-studio-2019>)

**Generate the Certificates**

Create the files that contain the CA certificate (root-ca.crt) & Signer certificate (signer-ca.crt). Navigate to the folder \CertGen\cert and execute the following scripts:

1. Create root-ca.crt & root-ca.key

> python ca\_create\_root.py

2. Create signer-ca.csr & signer-ca.key

> python ca\_create\_signer\_csr.py

3. Create signer-ca.crt

> python ca\_create\_signer.py

**Provisioning the ATWINC15x0**

1. Connect the SAM-IoT board to the PC (a disk drive named “CURIOSITY” should appear on the desktop and/or in a file explorer window)

A screenshot of a cell phone

Description automatically generated

1. Using a terminal emulator program, control panel, etc. – note the COM port number corresponding to the SAM-IoT board connection (most likely the device name will show up as something like “USB Serial Device”). Do **not** initiate any serial connection at this time if using a terminal emulator, e.g.

A screenshot of a cell phone

Description automatically generated

1. Drag & drop (i.e. copy) the “SAM\_IoT\_CertGen.hex” file to the “CURIOSITY” drive

|  |
| --- |
| **NOTE** |
| If the drag-and-drop operation fails, please refer to the instructions in “Drag and Drop Troubleshooting for SAM-IoT.docx”. If drag and drop still does not work, use a DOS command line to manually copy the file to the Curiosity drive letter. |

1. From the command line, go up one level to the “.\CertGen\” directory
2. Execute the following Python script:

> python provision\_samiot.py com<#>

(e.g. com<#> = com3)

This command should result in the following sequence of events:

1. MCU sends a request to the ECC to create a device Certificate Signing Request (CSR) (device.csr)
2. ECC signs the CSR with the signer’s private key (signer-ca.key)
3. ECC sends the device & signer certificates (device.crt & signer-ca.crt) back to the MCU
4. MCU copies the 2 certs into the ATWINC15x0’s flash memory

**Conclusion**

A total of 4 files are generated (device.csr, device.crt, signer-ca.key, signer-ca.crt) and 2 certificates (device.crt & signer-ca.crt) are stored in the ATWINC15x0

A screenshot of a computer

Description automatically generated

**Sample Output**

The following shows example certificates generated for a SAM-IoT board that has an ATECC608A which was pre-programmed with serial number 01239E946F011C66FE

An online tool such as a Certificate Decoder can be used to display the pertinent information for a particular certificate by simply pasting the text of the certificate into a browser: <https://www.sslshopper.com/certificate-decoder.html>

Root CA

A picture containing bird

Description automatically generated

Signer CA

A screenshot of a cell phone

Description automatically generated

Device

A picture containing bird

Description automatically generated

**APPENDIX A: Background Information**

1. MPLAB X Project “**SAM\_IOT\_WINC\_PROV\_Azure.X**” (located in the SAM\_IoT\_Certs\_Generator folder)

A screenshot of a social media post

Description automatically generated

This ATSAMD21 MCU-based project is made to run on the SAM-IoT board when the ECC608A is already configured with PRIV/PUB keys and compressed CERT. This “helper utility app” will provision the ATWINC15x0 with either the original ECC device certificate or create a new one using the ECC PRIV/PUB keys. The HEX file generated for this project has been supplied for ease of programming the SAM-IoT board. The complete project with all the source code is provided in case any further customizations might be needed beyond what is currently supported.

1. Interaction between the main Python script and the **SAM\_IOT\_WINC\_PROV\_Azure** application running on the SAMD21

|  |  |  |
| --- | --- | --- |
| **Python script (**provision\_samiot.py**)**  \_Sends “<genCsr”  \_Verify CSR signature  \_Scripts generate Device Cert by signing the CSR with SIGNER\_CA Private Key  \_Save Device Cert into “device.crt”  \_Send “>caCert” with signer-ca.crt  \_Send “>devCert” with device.crt  \_Sends “xferCerts [“2”] | **🡪**  **🡨**  **🡪**  **🡨**  **🡪**  **🡨**  **🡪** | **SAM\_IOT\_WINC\_PROV\_Azure**  \_Generate CSR from template “g\_csr\_def\_3\_device”  \_Derive public Key from private Key  \_Insert Public Key into CSR  \_Get CSR Digest  \_Sign Digest with Private Key  \_Insert Signed Digest into CSR  \_Return CSR to Python scripts  \_Receive ”caCert” and signer-ca.crt and stores it into buffer  \_Return SUCCESS  \_Receive ”devCert” with device.crt and stores it into buffer  \_Return SUCCESS  \_Copy “caCert” and “devCert” into WINC Flash |

**APPENDIX B: Creating Custom Templates**

The project needs to be built using the “ARM GNU Toolchain for 32-bit devices”: <https://www.microchip.com/mplab/avr-support/avr-and-arm-toolchains-c-compilers>

There are 3 templates used in the provisioning project:

1. Signer Certificate template

g\_cert\_template\_1\_signer[]

1. Device Certificate template

g\_cert\_template\_2\_device[]

1. Device Certificate Signing Request template

g\_csr\_template\_3\_device[]

To generate these templates, you need one of each (**signer-ca.csr**, **device.csr**, & **device.crt**). The **signer-ca.csr** was generated when you created the certificate earlier. For the **device.csr** and **device.crt** you will need to generate 2 samples.

To modify the Subject Common Name (CN) or the Subject Organization (O), look into the two (2) Python CSR generation for the following “x509.oid.NameOID.ORGANIZATION\_NAME” and “x509.oid.NameOID.COMMON\_NAME”. Change the name for your specific value and then save the files.

A close up of a screen

Description automatically generated

**Don’t forget** to regenerate the **signer-ca.crt** if you change its OID in the **signer-ca.csr**

Now you need to generate the 2 samples for **device.csr** & **device.crt**. Navigate to the folder “.\CertGen\cert” and run the following scripts:

1. python ca\_create\_device\_csr.py

(this will create device.csr)

1. python ca\_create\_device.py

(this will create device.crt)

At this point we should have 3 files: **signer-ca.crt,**  **device.csr**, and **device.crt** . Navigate to the folder “\CertGen\cert” and execute the following scripts:

1. python cert2certdef.py –signer-cert signer-ca.crt > signer-ca.c
2. python cert2certdef.py –device-csrt device.csr > device-csr.c
3. python cert2certdef.py –device-cert device.crt > device-crt.c

Open the 3 C files and copy each corresponding file’s contents into its corresponding C file in the **SAM\_IOT\_WINC\_PROV** project:

1. signer-ca.c 🡪 cert\_def\_1\_signer.c
2. device-csr.c 🡪 cert\_def\_3\_device\_csr.c
3. device-crt.c 🡪 cert\_def\_2\_device.c